|  |  |  |  |
| --- | --- | --- | --- |
| COIL PART NUMBER | RESISTANCE(s) | FUNCTION(s) | TENSION |
| A-489 | 15 OHMS | ADVANCE UNIT RELAY | 25 Volts |
| BALL GATE RELAY |
| 00-90 UNIT RELAY (MATCH UNIT) |
| A-1118 | 3.5 OHMS | BONUS INCREASE RELAY | 25 Volts |
| CONTROL BANK |
| DOUBLE BONUS RELAY |
| EXTRA BALL RELAY |
| 1st BALL RELAY |
| GAME OVER RELAY |
| LAST BALL RELAY |
| RESET CONTROL RELAY |
| 2nd,3rd,4th PLAYER RELAY |
| A-1119 | 2 OHMS | ROLLOVER RELAY | 25 Volts |
| A-1469 | 3 OHMS | GENERAL PURPOSE | 25 Volts |
| A-1496 | 3 OHMS | STEP-UP BALL PLAYER | 25 Volts |
| STEP-UP BONUS UNIT |
| STEP-UP PLAYER UNIT |
| STEP-UP REPLAY UNIT |
| BALL RETURN |
| BALL SHOOTER |
| HOLE KICKER |
| KICKING RUBBER |
| KICKING TARGET |
| POP BUMPER |
| 0-9 UNIT |
| A-4893 | 2 OHMS | BALL KICKER | 25 Volts |
| POP BUMPER |
| UP KICKER |
| A-5141 | 1 OHM / 8 OHMS | FLIPPER FLIPPER | 25 Volts |
| A-5143 | 3 OHMS | BELL BELL | 25 Volts |
| KNOCKER KNOCKER |
| A-5193 | 5 OHMS | SCORING | 25 Volts |
| A-5194 | 4.5 OHMS | STEP-UP BONUS UNIT | 25 Volts |
| STEP-UP COIN UNIT |
| STEP-UP CORNER UNIT |
| STEP-UP PLAYER UNIT |
| STEP-UP REPLAY UNIT |
| FLIPPER |
| GONG |
| HOLE KICKER |
| HOLE KICKING RUBBER |
| TARGET KICKING |
| TARGET KNOCKER |
| KNOCKER POP |
| BUMPER POP |
| BALL PLAYER RESET |
| COIN UNIT |
| CORNER UNIT RESET |
| SUBTRACT BONUS UNIT |
| REPLAY UNIT |
| SUBTRACT REPLAY UNIT |
| UP KICKER |
|   |
| COIL PART NUMBER | RESISTANCE(s) | FUNCTIONS | TENSION |
| A-5195 | 12 OHMS | BALL RELEASE | 25 Volts |
| CHIME |
| CONTACT KICKER |
| KNOCKER |
| OUTHOLE |
| A-5196 | 13 OHMS | CONTROL BANK RESET | 110 Volts |
| TARGET BANK RESET |
| A-5197 | ? ? | ROTO UNIT ROTO UNIT | 25 Volts |
| A-5294 | ? ? | 2 COINS PER PLAY RELAY | 110 Volts |
| A-5662 | 7,5 OHMS | LAST BALL RELAY | 25 Volts |
| LOCK RELAY |
| RESET CONTROL RELAY |
| A-6698 | 10,5 OHMS | 2 COINS, 3 PLAYS RELAY | 25 Volts |
| A-7677 | 0,5 OHM | COIN LOCKOUT | 25 Volts |
| A-7800 | 1 OHM | CONTROL BANK RESET | 25 Volts |
| A-7833 | 390 OHMS | GENERAL PURPOSE | 110 Volts |
| A-9154 | 6,5 OHMS | SCORING UNIT | 25 Volts |
| A-9479 | 21,5 OHMS | SEQUENCE BANK RESET | 110 Volts |
| TARGET RESET BANK (50 HZ) |
| A-9731 | ? ? | COIN CHUTE RELAY | 110 Volts |
| A-9733 | 2 OHMS | SERIES RELAY | 25 Volts |
| A-9735 | 14 OHMS | STEP-UP BONUS UNIT RELAY | 25 Volts |
| STEP-UP PLAYER UNIT RELAY |
| STEP-UP REPLAY UNIT |
| BALL RETURN RELAY |
| BALL SHOOTER RELAY |
| BONUS SCORE RELAY |
| CONTROL BANK RESET |
| HOLE VALUE RELAY |
| LAST BALL RELAY |
| PLAYERS RESET RELAY |
| POP BUMPER RELAY |
| RESET CONTROL RELAY |
| SCORE CONTROL RELAY |
| SPIN TARGET RELAY |
| START RELAY |
| 10-100-500-1000 POINTS RELAY |
| A-9736 | 25,5 OHMS | ALTERNATING RELAY | 25 Volts |
| COIN LOCKOUT |
| EXTRA BALL RELAY |
| 1st BALL RELAY |
| GAME OVER RELAY |
| HOLD RELAY |
|   |
| COIL PART NUMBER | RESISTANCE(s) | FUNCTION(s) | TENSION |
| A-9738 | 30 OHMS | ALTERNATING RELAY | 25 Volts |
| 115 VOLT RELAY |
| EXTRA BALL RELAY |
| HOLD RELAY |
| 100,000 POINTS RELAY |
| 30 VOLTS HOLD RELAY |
| TILT HOLD RELAY |
| A-9740 | 20 OHMS | "A","B","C", RELAY | 25 Volts |
| STEP-UP REPLAY UNIT |
| BONUS BOOSTER RELAY |
| BONUS SCORE CONTROL |
| 1st BALL RELAY |
| 1st,2nd,3rd, CHUTE RELAY |
| GAME OVER RELAY |
| REPLAY BUTTON RELAY |
| SEQUENCE COMPLETED RELAY |
| START RELAY |
| 3rd CHUTE DELAY RELAY |
| VARI - TARGET RESET |
| A-9741 | ? ? | REPLAY BUTTON RELAY | 110 Volts |
| 2 PLAY RELAY |
| A-9742 | 11 OHMS | TILT RELAY | 25 Volts |
| A-9746 | 2 OHMS | DOUBLE BONUS RELAY | 25 Volts |
| SERIES RELAY |
| A-12092 | ? ? | CHIME | 25 Volts |
| A-15259 | 7.5 OHMS | SCORING UNIT | 25 Volts |
| A-15359 | 0.5 OHM | DOUBLE BONUS CONTROL RELAY | 25 Volts |
| EXTRA BONUS RELAY |
| A-15555 | 9.5 OHMS | TARGET RESET BANK (60 HZ) | 110 Volts |
| A-16570 | 15.5 OHMS | KICKOUT HOLE | 25 Volts |
| OUTHOLE |
| A-16890 | 230 OHMS | ALTERNATING RELAY | 25 Volts |
| COIN LOCKOUT |
| EXTRA BALL RELAY |
| GAME OVER RELAY |
| TILT RELAY |
| A-17564 | 156 OHMS | VARI-TARGET | 25 Volts |
| A-17875 | 3 OHMS / 40 OHMS | FLIPPER | 25 Volts |
| A-17876 | 24 OHMS 24 OHMS | CHIME | 25 Volts |
| A-17891 | 3,5 OHMS 3.5 OHMS | ROTO UNIT ROTO UNIT | 25 Volts |
| TARGET BANK RESET (5 pos.) |
| A-18102 | 9 OHMS | TARGET RESET BANK (7 pos.) | 25 Volts |
|   |
| COIL PART NUMBER | COIL RESISTANCE(s) | FUNCTION(s) | TENSION |
| A-18318 | 7 OHMS | BANK TARGET RESET (4 pos.) | 25 Volts |
| A-18642 | 58 OHMS | MEMORY / DROP TARGET TRIP | 25 Volts |
| A-19217 | 25.5 OHMS | DROP TARGET TRIP (Pinball Pool) | 25 Volts |
| A-19300 | 8 OHMS | BALL KICKER | 25 Volts |
| A-19508 | 35 OHMS | DROP TARGET TRIP | 25 Volts |
| A-20095 | 2 OHMS / 35 OHMS | SUPER FLIPPER | 25 Volts |
| A-20558 | 156 OHMS | GATE GATE | 25 Volts |
| A-21741 | 2,5 OHMS 2.5 OHMS | UP KICKER | 25 Volts |
| A-24161 | 2 OHMS / 40 OHMS | INTERMEDIATE FLIPPER | 25 Volts |
| A-25959 | 4 OHMS / 202 OHMS | FLIPPER (New unit) | 25 Volts |
| A-26450 | 42 OHMS 42 OHMS | GENERAL PURPOSE | 25 Volts |
| A-26451 | 66 OHMS 66 OHMS | GENERAL PURPOSE | 25 Volts |
| A-26452 | 137 OHMS 137 OHMS | DROP TARGET TRIP | 25 Volts |
| A-26646 | 5 OHMS / 201 OHMS | FLIPPER (New Unit) | 25 Volts |
| A-26649 | 28,5 OHMS | GENERAL PURPOSE | 25 Volts |
| A-26926 | 33 OHMS | BANK TARGET RESET | 25 Volts |
| A-27642 | 9 OHMS / 203 OHMS | FLIPPER (New Unit) | 25 Volts |
| A-27643 | 11 OHMS / 202 OHMS | FLIPPER ( Old unit ) | 25 Volts |
| A-27926 | 65 OHMS | GENERAL PURPOSE | 25 Volts |
| **Electro-Magnetic Coils** |